VOLUNTARY CERTIFICATION SYSTEM

Assessment Center of Technical Competence

Registration No. ROSS RU.31459.04IDV0

**CERTIFICATE OF CONFORMITY**

 No. TsOTK.RU.PB002.N.00187 000774

 Number of Certificate of Conformity Form shelf number

|  |  |
| --- | --- |
| **APPLICANT**(Name and location of applicant) | Limited liability company "VIRMAK", OGRN 1142311012579, Legal address: 350916, Krasnodar Region, Krasnodar, Elizavetinskaya village, Tsentralnaya Street, bld. 209, RUSSIA. Business address: 353210, Krasnodar Region, Dinskoy District, Novotitarovskaya village, Lunacharskogo St., bld. 401B/3, RUSSIA, phone: +79182341412, e-mail: virmak23@mail.ru |
| **MANUFACTURER**(Name and location of the product manufacturer) | Limited liability company "VIRMAK", Legal address: 350916, Krasnodar Region, Krasnodar, Elizavetinskaya village, Tsentralnaya Street, bld. 209, RUSSIA. Business address: 353210, Krasnodar Region, Dinskoy District, Novotitarovskaya village, Lunacharskogo St., bld. 401B/3, RUSSIA, phone: +79182341412, e-mail: virmak23@mail.ru |
| **CERTIFYING BODY**(Name and location of Certifying body that issued Certificate of Conformity) | Certifying Body Limited Liability Company “Lanta Center” (CB LLC Lanta Center), 115088, Moscow, Sharikopodshipnikovskaya St. 4, bld. 4, phone +7(495) 675-85-81, fax +7(495) 675-85-81, OGRN 1137746804612, Certificate No. TsOTK IDV0.RU.OS.PR002 [ЦОТК ИДВ0.RU.ОС.ПР002] dated 13.05.2019 |
| **CERTIFIES THAT THE PRODUCT**(Identification of the certified products) | Structural insulation panels made of cement bonded particleboards with thickness from 10mm to 12mm from both sides and inner layer of thermal insulating material made of crude minerals flux of ISOVER, model “Sandwich LIFE” with thickness from 80mm to 250mm and density from 59 kg/m3 to 69 kg/m3 manufactured as per TU (Technical Specifications) 23.61.11-001-26412591-2017. Batch production | Russian Classification of Products by Economic Activities 2: 23.61.11.120EAEU Commodity Nomenclature of Foreign Economic Activity: 6811820000 |
| **CONFORMS TO REQUIREMENTS**(Identification of national standards, organization’s standards, set of rules, terms of contracts as of which the conformity of products is certified ) | GOST 30247.1-94. Structural units. Methods of fire-resistance tests. Bearing and enclosing structures. Fire resistance limit – E160  |
| **CONDUCTED EXAMINATIONS (TESTS) AND MEASUREMENTS** | Tests report No. D20-09-22/1 dated 22.09.2020Testing laboratory Lanta Center LLC, Certificate No. TsOTK IDV0.RU.IL.PR002 [ЦОТК ИДВ0.RU.ИЛ.ПР002] dated 13.05.2019, 115088, Moscow, Sharikopodshipnikovskaya St. 4, bld. 4 |
| **SUBMITTED DOCUMENTS**(Documents submitted by Applicant to Certifying Body as a proof of products conformity) | Quality Management System Certificate GOST R ISO 9001-2015 No. ST.RU.0001.P42810 dated 02.07.2020 issued by Certifying Body LLC “Garantiya Kachestva”, reg. No. ROSS RU.31389.04IBS01 |
| **DURATION OF VALIDITY OF CONFORMITY CERTIFICATE** |  from 23.09.2020 to 22.09.2025 |

*/Certifying body’s stamp/*

**Head (Deputy Head) of certifying body** */Signature/* **M.S.Zerkov**

**Expert (experts)** */Signature/* **D.Yu.Leonov**